<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.42.2-Münster">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>BOUNDCRS[SOURCECRS[PROJCRS["ETRS89 / Poland CS92",BASEGEOGCRS["ETRS89",DATUM["European Terrestrial Reference System 1989",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4258]],CONVERSION["unnamed",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",19,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9993,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",-5300000,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],ID["EPSG",2180]]],TARGETCRS[GEOGCRS["WGS 84",DATUM["World Geodetic System 1984",ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]]],ABRIDGEDTRANSFORMATION["Transformation from ETRS89 to WGS84",METHOD["Position Vector transformation (geog2D domain)",ID["EPSG",9606]],PARAMETER["X-axis translation",0,ID["EPSG",8605]],PARAMETER["Y-axis translation",0,ID["EPSG",8606]],PARAMETER["Z-axis translation",0,ID["EPSG",8607]],PARAMETER["X-axis rotation",0,ID["EPSG",8608]],PARAMETER["Y-axis rotation",0,ID["EPSG",8609]],PARAMETER["Z-axis rotation",0,ID["EPSG",8610]],PARAMETER["Scale difference",1,ID["EPSG",8611]]]]</wkt>
      <proj4>+proj=tmerc +lat_0=0 +lon_0=19 +k=0.9993 +x_0=500000 +y_0=-5300000 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs +type=crs</proj4>
      <srsid>0</srsid>
      <srid>0</srid>
      <authid></authid>
      <description>ETRS89 / Poland CS92</description>
      <projectionacronym></projectionacronym>
      <ellipsoidacronym>PARAMETER:6378137:6356752.31414035614579916</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
